

Software Safety Requirements and Architecture

Lane Assistance

**Document Version: 1.0**

**Template Version 2.0, Released on 2017-10-17**



Document History

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Editor | Description |
| 2017-10-16 | 1.0 | Daniel Gattringer | Initial version |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

Table of Contents

[Document History 2](#_Toc496105131)

[Table of Contents 2](#_Toc496105132)

[1. Purpose 3](#_Toc496105133)

[2. Inputs to the Software Requirements and Architecture Document 3](#_Toc496105134)

[2.1. Technical safety requirements 3](#_Toc496105135)

[2.2. Refined Architecture Diagram from the Technical Safety Concept 4](#_Toc496105136)

[3. Software Requirements 4](#_Toc496105137)

[4. Refined Architecture Diagram 9](#_Toc496105138)

# Purpose

The creation of Software Safety Requirements and the refining of the architecture are part of the safety process of ISO 26262 for the treatment of potential malfunctions in electrical and electronic systems.

The purpose of the Software Safety Requirements and the refining of the architecture is to identify new detailed software requirements and allocate them to component level diagrams of the lane assistance functional safety project.

# Inputs to the Software Requirements and Architecture Document

**REQUIRED:**

**You are only required to develop this document for the LDW (lane departure warning) amplitude malfunction. So here, provide the technical safety requirements for the LDW amplitude malfunction as well as the refined system architecture diagram from the technical safety concept.**

## Technical safety requirements

Technical Safety Requirements related to Functional Safety Requirement 01-01 are:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Architecture Allocation** | **Safe State** |
| Technical  Safety  Requirement  01-01-01 | The LDW safety component shall ensure that the amplitude of the ‘LDW\_Torque\_Request’ sent to the ‘Final electronic power steering Torque’ component is below ‘Max\_Torque\_Amplitude’ | C | 50ms | EPS ECU -LDW Safety  Component | Set the oscillating torque to zero. |
| Technical  Safety  Requirement  01-01-02 | As soon as the LDW function deactivates the LDW feature, the ‘LDW Safety’ software block shall send a signal to the car display ECU to turn on a warning light. | C | 50ms | EPS ECU -LDW Safety  Component | Set the oscillating torque to zero. |
| Technical  Safety  Requirement  01-01-03 | As soon as a failure is detected by the LDW function, it shall deactivate the LDW feature and the ‘LDW\_Torque\_Request’ shall be set to zero. | C | 50ms | EPS ECU -LDW Safety  Component | Set the oscillating torque to zero. |
| Technical  Safety  Requirement  01-01-04 | The validity and integrity of the data transmission for ‘LDW\_Torque\_Request’ signal shall be ensured. | C | 50ms | EPS ECU – Data Transmission Integrity Check | Set the oscillating torque to zero. |
| Technical  Safety  Requirement  01-01-05 | Memory test shall be conducted at startup of the EPS ECU to check for any faults in memory. | A | Ignition cycle | EPS ECU –  Safety Startup | Set the oscillating torque to zero. |

## Refined Architecture Diagram from the Technical Safety Concept

The following images shows the refined system architecture:

****

Technical overview of architecture elements:

|  |  |
| --- | --- |
| **Element** | **Description** |
| Camera Sensor | Sensor for the optical detection of the front area of the vehicle, including detectable lane lines. |
| Camera Sensor ECU | Electronic Control Unit responsible for detecting lane lines and determining when the vehicle leaves the lane by mistake. Responsible for triggering reactions to add extra torque for LDW and LKA functionality. |
| Camera Sensor ECU  Lane Sensing | Component within the camera sensor ECU responsible for detecting lane lines and determining when the vehicle leaves the lane by mistake. |
| Camera Sensor ECU Torque Request Generator | Component within the camera sensor ECU responsible for calculating and sending an request for additional steering torque for the LDW and LKA functionality. |
| Car Display | Visual display which is, among other functionalities, responsible for displaying warning of lane departures and LKA and LDW activation-status. |
| Car Display ECU | Electronic control unit, which is responsible for creating and providing the data and information that the car display visualizes. |
| Car Display ECU  LA on/off status | Component within the car display ECU responsible for visualizing if the lane assistance functionality is switched on or off. |
| Car Display ECU  LA active/inactive | Component within the car display ECU responsible for visualizing if the lane assistance functionality is active at the moment. Active means the car is drifting away from the center of the lane and LKA is actively acting or the car is getting too narrow to a lane boundary and LDW is warning. |
| Car Display ECU  LA malfunction warning | Component within the car display ECU responsible for visualizing if there occurs any malfunction within the lane assistance system. |
| Driver Steering Torque Sensor | Sensor responsible for measuring the steering torque provided by the driver. |
| Electronic Power Steering (EPS) ECU | The electronic control unit is responsible for evaluating the torque provided by the driver and for adding an additional torque based on the torque request of the lane assist system (LKA). Initializes the vibration of the steering wheel when the driver inadvertently drifts away from the center of the lane (LDW). |
| EPS ECU  Normal Lane Assistance Functionality | Component within the electronic power steering ECU responsible for receiving extra torque request from the camera sensor ECU and doing different non-safety tasks. |
| EPS ECU  Driver Steering Torque | Component within the electronic power steering ECU responsible for receiving the steering torque with which the driver moves the steering wheel. |
| EPS ECU  LDW Safety Functionality | Component within the electronic power steering ECU responsible for keeping the lane departure warning action (oscillating torque) below Max\_Torque\_Amplitude and Max\_Torque\_Frequency.  This component is also responsible for ensuring that the lane departure warning by means of vibration of the steering wheel is only applicated when LDW\_On is set. |
| EPS ECU  LKA Safety Functionality | Component within the electronic power steering ECU responsible for ensuring that the lane keeping assistance is not forcing the car longer than Max\_Duration to the center of the lane.  This component is also responsible for ensuring that the lane keeping assistance by forcing the car to the center of the lane is only applicated when the lane boundaries can be detected reliably. |
| EPS ECU  Final Torque | Component within the electronic power steering ECU responsible for ensuring that the single torque values from LDW, LKA are combined with the drivers original steering torque and sent to the motor. |
| EPS ECU  Safety Startup  Memory Test | Component within the electronic power steering ECU responsible for the memory test conducted at startup of the EPS ECU to check for any faults in memory. |
| EPS ECU  Data Transmission Integrity Check | Component within the electronic power steering ECU responsible for checking the data validity and integrity of the data transmission. |
| Motor | Mechatronic device which adds extra steering torque directly to the steering wheel. |

# Software Requirements

**Lane Departure Warning (LDW) Amplitude Malfunction Software Requirements:**

**[Instructions: Fill in the software safety requirements for the LDW amplitude malfunction technical safety requirements. We have provided the associated technical safety requirements. Hint: The software safety requirements were discussed in the text from the software and hardware lesson.**

Technical Safety Requirement 01-01-01 with its associated parameters

(derived in the technical safety concept):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-01 | The LDW safety component shall ensure that the amplitude of the ‘LDW\_Torque\_Request’ sent to the ‘Final electronic power steering Torque’ component is below ‘Max\_Torque\_Amplitude’ | C | 50ms | EPS ECU -LDW Safety  Component | Set the oscillating torque to zero. |

The following image shows the LDW safety component of the EPS ECU:



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ID | Software Safety Requirement | ASIL | Allocation Software Elements | Safe State |
| Software  Safety  Requirement  01-01 |  |  |  |  |
| Software Safety Requirement 01-02 |  |  |  |  |
| Software Safety Requirement 01-03 |  |  |  |  |

Technical Safety Requirement 01-01-02 with its associated parameters

(derived in the technical safety concept):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-02 | As soon as the LDW function deactivates the LDW feature, the ‘LDW Safety’ software block shall send a signal to the car display ECU to turn on a warning light. | C | 50ms | EPS ECU -LDW Safety  Component | Set the oscillating torque to zero. |

The following image shows the LDW safety component of the EPS ECU:



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 02-01 |  |  |  |  |
| Software Safety Requirement 02-02 |  |  |  |  |

Technical Safety Requirement 01-01-03 with its associated parameters

(derived in the technical safety concept):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-03 | As soon as a failure is detected by the LDW function, it shall deactivate the LDW feature and the ‘LDW\_Torque\_Request’ shall be set to zero. | C | 50ms | EPS ECU -LDW Safety  Component | Set the oscillating torque to zero. |

The following image shows the LDW safety component of the EPS ECU:



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement03-01 |  |  |  |  |
| Software Safety Requirement03-02 |  |  |  |  |
| Software Safety Requirement03-03 |  |  |  |  |
| Software Safety Requirement03-04 |  |  |  |  |
| Software Safety Requirement03-05 |  |  |  |  |

Technical Safety Requirement 01-01-04 with its associated parameters

(derived in the technical safety concept):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-04 | The validity and integrity of the data transmission for ‘LDW\_Torque\_Request’ signal shall be ensured. | C | 50ms | EPS ECU – Data Transmission Integrity Check | Set the oscillating torque to zero. |

The following image shows the LDW safety component of the EPS ECU:



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 04-01 |  |  |  |  |

Technical Safety Requirement 01-01-05 with its associated parameters

(derived in the technical safety concept):

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-05 | Memory test shall be conducted at startup of the EPS ECU to check for any faults in memory. | A | Ignition cycle | EPS ECU –  Safety Startup | Set the oscillating torque to zero. |

The following image shows the LDW safety component of the EPS ECU:



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 05-01 |  |  |  |  |
| Software Safety Requirement 05-02 |  |  |  |  |
| Software Safety Requirement 05-03 |  |  |  |  |
| Software Safety Requirement 05-04 |  |  |  |  |

# Refined Architecture Diagram

**[Instructions: Include the refined system architecture. Hint: The refined system architecture should include the system architecture from the end of the software and hardware lesson, including all of the ASIL labels.]**



# ../Architecture_Diagrams/graphic_asset_1.png